< Hálózat

Interfészek

Szerző: Sallai András

Copyright © 2020, Sallai András

Licenc: CC BY-SA 4.0

Web: https://szit.hu

Hálózati kártya nevek

lo - Loopback, visszacsatoló eszköz

eth0 - Ethernet kártya

pan0 - Personal Area Network - Bluetooth

vboxnet0 - VirtualBox virtuális hálózati kártyája

wlan0 - Wifi eszköz

wmaster0 - Wifi eszköz

ra0 - wireless

ppp0 - Modem, pont-pont-kapcsolat

Példa

A kimenet például ilyen lehet:

1: lo: <LOOPBACK,UP,LOWER_UP> mtu 16436 qdisc noqueue state UNKNOWN
link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
inet6 ::1/128 scope host
valid_lft forever preferred_lft forever
2: eth0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc pfifo_fast state UNKNOWN qlen 1000
link/ether 00:50:8d:7c:ab:04 brd ff:ff:ff:ff:ff:ff
inet 192.168.1.4/24 brd 192.168.1.255 scope global eth0
inet6 fe80::250:8dff:fe7c:ab04/64 scope link
valid_lft forever preferred_lft forever
3: pan0: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN
link/ether f2:b4:8f:e4:8e:77 brd ff:ff:ff:ff:ff:ff
4: vboxnet0: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN qlen 1000
link/ether 0a:00:27:00:00:00 brd ff:ff:ff:ff:ff:ff